MENSAJE NAVAL OPERATIVO

PRIORIDAD 070810 NOV 2025		RESERVADO		TA ORIGEN: LATORRE 
          
DEL: LATORRE
AL: PRAT	 
(F): CENTARM     ESCUADRAADM

ETAPA PRACTICA CIGN 2025 / OPERATION FORGE / OPTASK RAS
OPER/CIGN 2025/OPERATION FORGE//
MSGID/OPTASK RAS/APP-11(D)/1/LATORRE/001/NOV// 
REF/A/DOC/APP-11(D)(1)/NOV2015//
REF/B/PUB/ATP-1 (I)(1) VOL II/NATO/DIC2020/1/-I-I/
REF/C/DOC/NTTP 4-01.4/MAR2009/UNDERWAY REPLENISHMENT/
REF/D/DOC/ATP/MTP-16 REPLENISHMENT AT SEA(F)(1)/MAY 2016/ 
REF/E/MSG/OPERATION FORGE OPGEN/LATORRE/061601P4NOV2025//
REF/F/MSG/OPTASK COMMS/ESCUADRAADM/071204P4FEB2025/001//

GEODATUM/WGE//
PERIOD/110800P0NOV2025/141200P8NOV2025// 
RASRDVU/TBD//
MLA/TBD IAW SITAC//
RASFORM/TBD//
RASDET/LATORRE - ONE - STARBOARD/LIGHT JACK STAY/ PRAT – TWO – PORT/LIGHT JACK STAY//
LIFEGUARD/TBD/
DUTY/TBD/
GENTEXT/EMERGENCY BREAKAWAY ORDERED ONLY BY CO'S//
GENTEXT/SPECINST/1/ALTERATION OF COURSE AND SPEED WILL BE BY METHOD BRAVO IAW REF B (VOICE)/
GENTEXT/SPECINST/2/RAS MINIMUM VISIBILITY REQUIREMENT 1000 YDS//
GENTEXT/SPECINST/3/GYRO CROSS CHECK WILL BE CONDUCTED BY RECEIVING SHIP AND EXECUTED ONLY WHEN RECEIVING SHIP INDICATES "READY"/GYRO CROSS CHECK WILL BY EXECUTED BY PRITAC COMMS//
GENTEXT/SPECINST/4/DURING RAS DISTANCE BETWEEN SHIPS WILL BE 42MTS6 (140FT5) TO FACILITATE SPANWIRE HANDLING/ MINIMUM DISTANCE BETWEEN SHIPS WILL BE 24MTS6 (80FT8) / MAXIMUM DISTANCE BETWEEN SHIPS WILL BE 61MTS7 (200FT2)// GENTEXT/SPECINST/5/APPROACHING METHOD/FAST APPROACH//
GENTEXT/SPECINST/6/FIRING SHIP WILL ATTEMPT A MAXIMUM OF TWO FIRINGS/ IF UNSUCCESSFUL DUTY 209 WILL BE REASSIGNED/ SHIPS WITH HELO ON DECK WILL ASSUME DUTY 209/
GENTEXT/SPECINST/8/COMMUNICATIONS IAW REF F/
/1/ PRITAC COMMS PRIMARY/TF-TG TACTICAL VHF/TA-10/D/PRESET G4 - 74.6M7(P)/-/J3E-WNSP/G-ALL//
/2/PRITAC COMMS ALTERNATIVE/TF-TG TACTICAL VHF/TA-10/E/PRESET G5 – 76.4M7(S)/-/ J3E-WNSP/AR//
/3/COMSUP COMMS PRIMARY/TF-TG ASUW-ASW COORD REPORT UHF/TA-200/D/HQ-II FMT ALFA-NET 08-A00.825(P)/J3E- WONSP/G-ALL//
/4/COMSUP COMMS ALTERNATIVE/TF-TG ASUW-ASW COORD REPORT UHF/TA-200/E/HQ-II FMT ALFA-NET 09-A00.925(S)/J3E- WONSP/AR//
/5/ALL UNITS/SAFETY OFFICERS COMMS/PRIMARY LINE TA 40X/CH-03 VHF// 
/6/ALL UNITS/STATIONS STATIONS PRIMARY HAND SIGNAL PADDLES/ALTERNATIVE SOUND POWERED PHONES/
/7/BRIDGE TO BRIDGE COMMS/PRIMARY SOUND-POWERED/
/8/ALTERNATIVE BRIDGE TO BRIDGE COMMS/LINE TA 40V/CH-01 VHF/
/9/ALL COMMS WILL BE CONDUCTED BY SECURE LINES/SECONDARY AND ALTERNATIVE LINE 40(-) VHF WILL BE USE ONLY AS LAST RESOURCE/
AKNLG/NO//

