MENSAJE LATORRE ENTRENAMIENTO 2023

EXER/ENTRENAMIENTO LATORRE 2023/REPLENISHMENT AT SEA//  
MSGID/OPTASK RAS/APP-11 (D)/LATORRE/1/20230807/NEW/1/-/RESTRICTED//  
REF/A/TYPE:PUB/NTTP 4-01.4/  
REF/B/TYPE:PUB/ATP-1(H)(1)VOL II/  
REF/C/TYPE:PUB/ATP-16 (D)/  
REF/D/TYPE:MSG/OPTASK COMMS/ESCUADRAADM/080730PMAR2023/001/  
REF/E/TYPE:MSG/EXORD 018/ENTRENAMIENTO LATORRE/ESCUADRAADM/191241QJUL2023/001//  
GEODATUM/WGE//  
PERIOD/040800QAUG2023/012359QSEP2023//  
AMPN/COMMS CHECKS TO START 30 MIN PRIOR TO RAS//  
RASRDVU/TBD BY MSG MISCEX 805//  
MLA/ TBD BY MSG MISCEX 805/REPLENISHMENT COURSE MAY BE CHANGE IAW SEA CONDITIONS//  
AMPN/INTENDED RAS SPEED 10 KTS//  
RASDET/ARAUCANO-ONE STARBOARD SIDE/LATORRE-FOUR PORT SIDE /SPANWIRE-PROBE/PELICAN HOOK//  
LIFEGUARD/TBD IAW MSG MISCEX 805//  
DUTY/UNIT:LATORRE/139/142/204/209/216/221/  
DUTY/UNIT:/ARAUCANO/136/140//  
GENTEXT/EMERGENCY BREAKAWAY ORDERED ONLY BY CO’S IAW SAFETY BRIEFING//  
GENTEXT/SPECINST/1/ALTERATION OF COURSE AND SPEED WILL BE BY METHOD BRAVO IAW REF B (RADIO)/  
GENTEXT/SPECINST/2/RAS MINIMUM VISIBILITY REQUIREMENT 1000YDS1/  
GENTEXT/SPECINST/3/GYRO CROSS CHECK WILL BE CONDUCTED BY RECEIVING SHIP AND EXECUTED ONLY 
WHEN ARAUCANO INDICATES "READY"/  
GENTEXT/SPECINST/4/DURING FAS DISTANCE BETWEEN SHIPS WILL BE 42 METERS (140FT) TO FACILITATE 
SPANWIRE HANDLING/MINIMUM DISTANCE BETWEEN SHIPS WILL BE 24 METERS (80 FT)/MAXIMUM DISTANCE 
BETWEEN SHIPS WILL BE 61 METERS (200 FT)/  
GENTEXT/SPECINST/5/FIRING SHIP WILL ATTEMPT A MAXIMUM OF TWO FIRINGS. IF UNSUCCESFUL DUTY 209 
WILL BE REASIGNED/  
GENTEXT/SPECINST/6/LATORRE/RAS CONDUCTIONS WILL BE BY PRITAC COMMS PRIMARY/  
GENTEXT/SPECINST/7/COMUNICATIONS/  
/1/PRITAC COMMS PRIMARY TA-100/E/76.4M7/CH-04/ ALTERNATIVE TA-100/F/65.3M4/CH-05/  
/2/COMSUP COMMS PRIMARY TA-200/E/FMT ALFA-NET 09-A00.925/ALTERNATIVE TA-200/F/FMT ALFA-NET 08-
A00.825/  
/3/BTB COMMS DELIVERING UNIT/PRIMARY SOUND-POWERED PHONE/SECONDARY LINE 40V/CH-01 
VHF/ALTERNATIVE LINE 40Y/CH-04 VHF/  
/4/SAFFETY OFFICERS COMMS LINE 40X/CH-03 VHF/SECONDARY LINE 40W/CH-02 VHF/ ALTERNATIVE LINE 40 
Q/CH-05 VHF/  
/5/STATION-STATION/PRIMARY HAND SIGNAL PADDLES/SECONDARY SOUND-POWERED PHONES/  
GENTEXT/SPECINST/8/RASREQ MUST BE SEND 12 HOURS BEFORE MANOUVER/  
GENTEXT/SPECINST/9/SRL WILL BE CONDUCTED IAW MISCEX 805//  
GENTEXT/SPECINFO/1/SAFETY BRIEFING WILL BE CONDUCTED IAW PARAGRAPH 2.2.11.4 (REF A)/  
GENTEXT/SPECINFO/2/SAFETY IS PARAMOUNT//  
AKNLDG/NO//
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MENSAJE ARAUCANO OPS 4-5
OPER/OPS 4-5 2025//   
MSGID/OPTASK RAS/APP-11(D)/ARAUCANO/003/NOV/NEW/1/NATO/UNCLASSIFIED/-//   
REF/A/DOC/APP-11(D)(1)/NOV2015//   
REF/B/PUB/ATP-1(I)(1) VOL II/NATO/DEC2020/1/-/-//   
REF/C/DOC/NTTP 4-01.4/MAR2009/UNDERWAY REPLENISHMENT//   
REF/D/DOC/ATP/MTP-16 REPLENISHMENT AT SEA(F)(1)/MAY 2016//   
REF/E/MSG/OPS 4-5/OPGEN/CUT 400.1.1 (CATF)/YAGAN/291150AUG2025//   
REF/F/MSG/OPS 4-5/SOE CGT 400.1 FASE I V1.0/SOBERANIA/291400AUG2025//   
REF/G/MSG/OPTASK COMMS SOBERANIA/ESCUADRAADM/281648AUG2025//   
GEODATUM/WGE//   
PERIOD/041900Q4SEP2025/312359Q3OCT2025//   
AMPN/COMMS CHECKS TO START 30 MIN PRIOR TO RAS//   
RASRDVU/TBD: IAW SITAC//   
MLA/ TBD BY MSG MISCEX 805/REPLENISHMENT COURSE MAY BE CHANGE IAW SEA CONDITIONS//   
AMPN/TBD BY OCE//   
RASFORM/TBD BY OCE//   
RASDET/ARAUCANO-ONE STARBOARD SIDE/SPANWIRE-PROBE/PELICAN HOOK/ARAUCANO-TWO PORT SIDE/LIGHT JACKSTAY/PELICAN HOOK//  
LIFEGUARD/TBD IAW SECUENCE MSG MISCEX 805//   
DUTY//IAW OPGEN CUT 400.1.1 (CATF)//   
GENTEXT/EMERGENCY BREAKAWAY ORDERED ONLY BY CO'S//   
GENTEXT/SPECINST/1/ALTERATION  OF  COURSE  AND  SPEED  WILL  BE  BY  METHOD  BRAVO  IAW  REF  B  (VOICE RADIO)//   
GENTEXT/SPECINST/2/RAS MINIMUM VISIBILITY REQUIREMENT 3000 YDS//   
GENTEXT/SPECINST/3/GYRO  CROSS  CHECK  WILL  BE  CONDUCTED  BY  RECEIVING  SHIP  AND  EXECUTED  ONLY WHEN ARAUCANO INDICATES "READY"/ GYRO CROSS CHECK WILL BY EXECUTED BY PRITAC COMMS PRIMARY//   
GENTEXT/SPECINST/4/DURING  RAS  DISTANCE  BETWEEN  SHIPS  WILL  BE  42  METERS  (140FT)  TO  FACILITATE SPANWIRE HANDLING/ MINIMUM DISTANCE BETWEEN SHIPS WILL BE 24 METERS (80FT)/ MAXIMUN DISTANCE 
BETWEEN SHIPS WILL BE 61 METERS (200FT)//   
GENTEXT/SPECINST/5/APPROACHING METHOD/ FAST APPROACH/ MEDIUM SPEED APROACH/ BEAM APPROACH/ TBD IAW WEATHER CONDITION//   
GENTEXT/SPECINST/6/FIRING SHIP WILL ATTEMPT A MAXIMUM OF TWO FIRINGS/ IF UNSUCCESSFUL DUTY 209 WILL BE REASIGNED/ SHIPS WITH HELO ON DECK WILL ASSUME DUTY 209//   
GENTEXT/SPECINST/7/CONSIDER UNITS SHOULD BE READY TO EXECUTE VISUAL SIGNALS EXERCISE (FLAGS OR FLASHES) ON ALL EV RAS//   
GENTEXT/SPECINST/8/COMUNICATIONS IAW REF G//   
/1/ PRITAC COMMS PRIMARY TA-10/COMMAND PRESET 1/N-1/43.9M6/VHF/J3E-FFLOS/CT/G-ALL//   
/2/ PRITAC COMMS ALTERNATIVE TA-10 /COMMAND PRESET 2/N-2/38.5M6/VHF/J3E-FFLOS/CT/AR//  
/3/COMSUP COMMS PRIMARY TA-200/D/HQ-II FMT ALFA-NET 08-A00.825 (P) /J3E- WONSP/G-ALL//   
/4/COMSUP COMMS ALTERNATIVE TA-200 / E / HQ-II FMT ALFA-NET 09-A00.925 (S) / J3E- WONSP / AR//   
/5/ALL UNITS/SAFFETY OFFICERS COMMS/PRIMARY LINE TA-40X/CH-03 VHF//   
/6/ALL UNITS/STATIONS STATIONS PRIMARY HAND SIGNAL PADDLES/ALTERNATIVE SOUND-POWERED PHONES//   
/7/BRIDGE  TO  BRIDGE  COMMS/PRIMARY  SOUND-POWERED  PHONE/SECONDARY  AND  ALTERNATIVE  IN  MSG MISCEX 805//   
/8/ALL COMMS WILL BE CONDUCTED BY SECURE LINES/SECUNDARY AND ALTERNATIVE LINE 40(-) VHF WILL BE USE ONLY AS LAST RESOURCE//   
GENTEXT/SPECINST/9/SRL WILL BE CONDUCTED IAW MISCEX 805//   
GENTEXT/SPECINST/10/UNITS SEND PRE-CRITIC MESSAGE IAW MSG MISCEX 805//   
GENTEXT/SPECINFO/1/SAFETY IS PARAMOUNT//   
AKNLDG/NO//
